# XPlaneConnect Toolbox-pauseSim

<-- Back

# pauseSim

## Inputs

- Pause: binary value 0=run, 1=pause
- IP Address (optional): IP Address of the machine that will receive the data as a character array. Default is '127.0.0.1' (local machine)
- port (optional): Port on the receiving machine where the data will be sent. Default is 49009 (XPlaneConnect). In general use 49009 to send to the plugin and 49005 to send to the x-plane udp

## Outputs

- status: If there was an error. status<0 means there was an error.

## Use

1. import XPlaneConnect.*;
2. status = pauseSim(1);

## Change Log

10/02/14: [CT] V0.9: Updated to work with updated xpcPlugin
06/10/13: [CT] Code created
<-- Back