# XPlaneConnect Toolbox-selectDATA

<-- Back

# selectDATA

Choose specific X-Plane parameters to be send over UDP

## Inputs

- index: An array of the values that to be sent. Corresponds to the numbers on the XPlane Output screen (ACTUAL NAME?)
- IP Address (optional): IP Address of the machine that will receive the data as a character array. Default is '127.0.0.1' (local machine)
- port (optional): Port on the receiving machine where the data will be sent. Default is 49009 (XPlaneConnect). In general use 49009 to send to the plugin and 49005 to send to the x-plane udp

## Outputs

- status: If there was an error. Status<0 means there was an error.

## Use

1. import XPlaneConnect.*;
2. values = [1, 2, 3, 27, 40]; 3. status = selectDATA(values,'127.0.0.1',49005);

## Change Log

10/02/14: [CT] V0.9: Updated to work with updated xpcPlugin
04/18/14: [CT] V0.2: Added Versioning
06/10/13: [CT] Code created
<-- Back