# XPlaneConnect Toolbox-requestDREF

<-- Back

# requestDREF

## Inputs

- DREFArray: Cell Array of DataRefs to be requested
- IP Address (optional): IP Address of the machine that will receive the data as a character array. Default is '127.0.0.1' (local machine)
- port (optional): Port on the receiving machine where the data will be sent. Default is 49009 (XPlaneConnect). In general use 49009 to send to the plugin

## Outputs

- status: If there was an error. status<0 means there was an error.

## Use

1. import XPlaneConnect.*;
2. DREFArray = {'sim/cockpit2/controls/yoke_heading_ratio','sim/cockpit2/controls/yoke_roll_ratio'};
3. status = requestDREF( DREFArray, '172.0.100.54' );

## Change Log

10/02/14: [CT] V0.9: Updated to work with updated xpcPlugin
06/10/13: [CT] Code created
<-- Back