# XPlaneConnect Toolbox-sendUDP

<-- Back

# sendUDP

Send an one dimensional array of type uint8 data over an UDP connection

## Inputs

- data: 1-D array of type uint8 data to be sent
- IP Address (optional): IP Address of the machine that will receive the data as a character array. Default is '127.0.0.1' (local machine)
- port (optional): Port on the receiving machine where the data will be sent. Default is 49009 (XPlaneConnect). In general use 49009 to send to the plugin and 49005 to send to the x-plane udp

## Outputs

- status: If there was an error. Status=1 means there was an error.

## Use

1. import XPlaneConnect.*;
2. data = uint8([1:20]);
3. #Send the data array to port 49005 on the computer at IP address 172.0.100.54.
4. status = sendUDP( data, '172.0.100.54', 49005 );

## Change Log

10/02/14: [CT] V0.9: Updated to work with updated xpcPlugin
06/10/13: [CT] Code created
<-- Back